
ReQuest Pronto RSU9600   Version 0.90 Beta

Installation notes:
1. This pronto file requires Pronto Professional Edit Version 1.1.20.0  Build Date: Jun 28, 2007
2. Save the .xcf file to the local hard drive. 
3. Open the ReQuest_Pronto_TSU9600_v0_90_beta.zcf file in Pronto Edit and copy and paste the "AudioReQuest" device into your project.
4. Modify Parameters page:

To modify parameters, double click the text box of the parameter, and select the 'label' tab.  

IP Address - This is the IP address of the AudioReQuest.  Make sure it is set to static and is outside of the DHCP range of the router

Port - This is the communications port of the AudioReQuest.  In mostly all cases it will be 3663. 

Default Zone - The zone that the Pronto connects to intially.  For instance, if you have Zone 2 dedicated to the upstairs, the upstairs Pronto would have a default zone of 2.

Total # of Zones - This is based on the number of audio outputs on the AudioReQuest.  N.Series = 1, F2.Series = 2,  F4.Series = 4, S.Series = 4

Allow Zone Switching - If you want the Pronto to be able to control other zones, set this to "true".  If not, set to "false".

Zone 1 name - Fill in the zone names. i.e. Upstairs, Kitchen, Yard etc.

